Comparison of NMR and EPOL

Method

ffl normalise NMR’s to first EPOL in fill ffl adjusted for average rise from end ramp to time of EPOL ffl ie all NMR’s calibrated to same energy at end of ramp ffl do this separately for a) NMR48 and b) all available ffl for plot re zero NMR after each mini-ramp ffl results for all rather sensitive to which probes included

Conclude : need more study and quality checks

Caveats

ffl tide correction still approximate ffl no account yet of effect of BOM during fill ffl no quantitative conclusions !

NoV. 7 1997 LEP Energy Meeting Pete Renton