N_{tracks}

Number of Events / Track

cut

cut

L3 Data qqτν M.C. signal M.C. background preliminary

192 - 202 GeV

0

100

200

300

0 1 2 3 4 5 6 7