year fill E_{nom} length t.a.r.^1 start day end day ΔE comment (h) (h) time (h) time (h) [MeV] 92 1439 Peak 6.5 7.5 11-11 11-11 0.9 Tide exp. I, 02:00 08:30 beams lost 1440 Peak 10.5 3.5 11-11 12-11 -0.7 Tide exp. I, 14:00 00:30 continued 93 1636 P-2 4 2.5 20-06 20-06 1.2 MD 17:00 21:00 1734 P-2 4.5 2 05-08 05-08 2.2 MD 00:00 04:30 1772 P-2 21.5 1.5 29-08 29-08 7.8 Tide exp. II, 02:40 24:00 temp. exp.

1811 P+2 5.5 21 12-09 12-09 -1.2 after physics 14:00 19:20 1849 P-2 11 13.5 11-10 12-10 3.5 Tide exp. III, 19:40 06:30 after physics 94 2234 Peak 10.5 12 25-07 25-07 0.5 jump in E_{fd}: 10:20 21:00 2.2 MeV 95 2929 P-2 9.5 4 24-08 25-08 1.9 MD 19:10 04:45 3022 P+2 16 1.5 24-09 25-09 3.4 BoF/BoF/EoF 18:30 10:15 calibr.

3029 P+2 15.5 2 28-09 29-09 6.5 BoF/EoF 19:00 10:30 calibr.

3030 P-2 21 1 29-09 30-09 4.4 BoF/EoF 17:00 14:00 calibr.

3036 P+2 16 1 02-10 02-10 1.7 BoF/EoF 01:00 17:00 calibr.

3064 P+2 7 1 08-10 08-10 1.4 MD 13:30 20:20

Table 1: Table of long term resonant depolarisation experiments since Nov. 1992. All calibration experiments with more than 4 h duration are included. Start and end time are the time of the first and last energy measurement respectively. No corrections apart from those for tidal effects are applied to the measured energy differences (ΔE) between the first and last measurement.

1 time after ramp to the final energy